What security level set to automatically when you set the nameif to inside

100

What able nameif outside? What is the security level?

0

Describe default communication allowed by the Cisco ASA simply by defining the security levels. A quick web search should help here. Example search: “security levels communicate cisco asa”

Higher security interface traffic to lower security interface is permitted

Lower to higher is denied

Same security is blocked

Why are pings not allowed when tcp is allowed as stateful traffic on your firewall

Pings use ICMP not TCP, so a specific rule is needed to permit them, as opposed to stateful rules which automatically handle returning TCP traffic for established connections.